(kicad_sch (version 20211123) (generator eeschema)
  (paper "A4")
  (title_block
    (title "Value field split test")
    (date "2023-05-03")
    (company "Instituto Nacional de Tecnología Industrial - CMNT")
    (comment 1 "KiBot")
  )
  (lib_symbols
    (symbol "Device:C" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "C" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 4) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 6) (at 0 0 0))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:L" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "L" (id 0) (at -1.27 0 90))
      (property "Value" "L" (id 1) (at 1.905 0 90))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "inductor choke coil reactor magnetic" (id 4) (at 0 0 0))
      (property "ki_description" "Inductor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Choke_* *Coil* Inductor_* L_*" (id 6) (at 0 0 0))
      (symbol "L_0_1"
        (arc (start 0 -2.54) (mid 0.635 -1.905) (end 0 -1.27)
          (fill (type none))
        )
        (arc (start 0 -1.27) (mid 0.635 -0.635) (end 0 0)
          (fill (type none))
        )
        (arc (start 0 0) (mid 0.635 0.635) (end 0 1.27)
          (fill (type none))
        )
        (arc (start 0 1.27) (mid 0.635 1.905) (end 0 2.54)
          (fill (type none))
        )
      )
      (symbol "L_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "1")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 2.032 0 90))
      (property "Value" "R" (id 1) (at 0 0 90))
      (property "Footprint" "" (id 2) (at -1.778 0 90))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "R res resistor" (id 4) (at 0 0 0))
      (property "ki_description" "Resistor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
  )
  (symbol (lib_id "Device:C") (at 76.2 54.61 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C1" (id 0) (at 79.121 53.4162 0))
    (property "Value" "1uF 0603 ±30%" (id 1) (at 79.121 55.7784 0))
    (property "Footprint" "" (id 2) (at 77.1652 58.42 0))
    (property "Datasheet" "~" (id 3) (at 76.2 54.61 0))
    (property "tolerance" "30%" (id 4) (at 79.121 58.0644 0))
    (property "package" "0603" (id 5) (at 79.121 60.3504 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 101.6 54.61 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "C2" (id 0) (at 104.521 53.4162 0))
    (property "Value" "100p 0805 NPO 50V" (id 1) (at 104.521 55.7784 0))
    (property "Footprint" "" (id 2) (at 102.5652 58.42 0))
    (property "Datasheet" "~" (id 3) (at 101.6 54.61 0))
    (property "voltage" "50 V" (id 4) (at 104.521 58.0644 0))
    (property "package" "0805" (id 5) (at 104.521 60.3504 0))
    (property "characteristic" "C0G" (id 6) (at 104.521 62.6364 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 76.2 67.31 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R1" (id 0) (at 77.978 66.1162 0))
    (property "Value" "12k 1% 0402 1/8W" (id 1) (at 77.978 68.4784 0))
    (property "Footprint" "" (id 2) (at 74.422 67.31 90))
    (property "Datasheet" "~" (id 3) (at 76.2 67.31 0))
    (property "tolerance" "1%" (id 4) (at 77.978 70.7644 0))
    (property "package" "0402" (id 5) (at 77.978 73.0504 0))
    (property "power" "125 mW" (id 6) (at 77.978 75.3364 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 101.6 67.31 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "R2" (id 0) (at 103.378 66.1162 0))
    (property "Value" "1M 10%" (id 1) (at 103.378 68.4784 0))
    (property "Footprint" "" (id 2) (at 99.822 67.31 90))
    (property "Datasheet" "~" (id 3) (at 101.6 67.31 0))
    (property "tolerance" "10%" (id 4) (at 101.6 67.31 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:L") (at 76.2 80.01 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "L1" (id 0) (at 77.597 78.8162 0))
    (property "Value" "3n3 0603 10%" (id 1) (at 77.597 81.1784 0))
    (property "Footprint" "" (id 2) (at 76.2 80.01 0))
    (property "Datasheet" "~" (id 3) (at 76.2 80.01 0))
    (property "tolerance" "10%" (id 4) (at 77.597 83.4644 0))
    (property "package" "0603" (id 5) (at 77.597 85.7504 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:L") (at 101.6 80.01 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "L2" (id 0) (at 103.0224 78.8162 0))
    (property "Value" "1nH 100V" (id 1) (at 103.0224 81.1784 0))
    (property "Footprint" "" (id 2) (at 101.6 80.01 0))
    (property "Datasheet" "~" (id 3) (at 101.6 80.01 0))
    (property "Voltage" "100 V" (id 4) (at 101.6 80.01 0))
    (pin "1")
    (pin "2")
  )
  (sheet_instances
    (path (page "1"))
  )
  (symbol_instances
    (path
      (reference "C1") (unit 1) (value "1uF 0603 ±30%") (footprint "")
    )
    (path
      (reference "C2") (unit 1) (value "100p 0805 NPO 50V") (footprint "")
    )
    (path
      (reference "L1") (unit 1) (value "3n3 0603 10%") (footprint "")
    )
    (path
      (reference "L2") (unit 1) (value "1nH 100V") (footprint "")
    )
    (path
      (reference "R1") (unit 1) (value "12k 1% 0402 1/8W") (footprint "")
    )
    (path
      (reference "R2") (unit 1) (value "1M 10%") (footprint "")
    )
  )
)
